int led = 13; // the pin that the LED is atteched to

int sensor = 2; // the pin that the sensor is atteched to

int state = LOW; // by default, no motion detected

int val = 0; // variable to store the sensor status (value)

void setup() {

pinMode(led, OUTPUT); // initalize LED as an output

pinMode(sensor, INPUT); // initialize sensor as an input

Serial.begin(9600); // initialize serial

}

void loop(){

val = digitalRead(sensor); // read sensor value

if (val == HIGH) { // check if the sensor is HIGH

digitalWrite(led, HIGH); // turn LED ON

delay(500); // delay 100 milliseconds

if (state == LOW) {

Serial.println("Motion detected!");

state = HIGH; // update variable state to HIGH

}

}

else {

digitalWrite(led, LOW); // turn LED OFF

delay(500); // delay 200 milliseconds

if (state == HIGH){

Serial.println("Motion stopped!");

state = LOW; // update variable state to LOW

}

}

}